Fastener Tightening Specifications. Chevrolet LUVW 2003

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Adapter Case Bolts | 36 N·m | 27 lb ft
Brake Apply Cover Bolts | 10 N·m | 89 lb in
Center Support Bolts | 26 N·m | 19 lb ft
Converter Housing Bolt Position A | 36 N·m | 27 lb ft
Converter Housing Bolt Position B | 58 N·m | 43 lb ft
Detent Spring Bolt | 5 N·m | 44 lb in
Fluid Filter Screen Bolts | 5 N·m | 44 lb in
Lower Valve Body Plate Bolts | 5 N·m | 44 lb in
Lower Valve Body Side Bolts | 5 N·m | 44 lb in
Manual Shaft Lever Nut | 13 N·m | 115 lb in
Oil Pump Bolts | 22 N·m | 16 lb ft
Oil Pump Cover-To-Oil Pump Body Bolts | 9 N·m | 80 lb in
Parking Pawl Plate Bolts | 7 N·m | 62 lb in
Pressure Relief Valve Bolts | 5 N·m | 44 lb in
Rear Valve Body Plate Bolts | 5 N·m | 44 lb in
Shift Solenoid Bolts | 10 N·m | 89 lb in
Speed Sensor Bolt | 23 N·m | 17 lb ft
TCC Control Valve Plate Bolts | 5 N·m | 44 lb in
TCC Solenoid Bolts | 5 N·m | 44 lb in
Transmission Oil Pan Bolts | 4 N·m | 35 lb in
Transmission Range Switch Bolt | 5 N·m | 44 lb in
Transmission Range Switch Set Nut | 5 N·m | 44 lb in
TV Cable Cam Bolt | 8 N·m | 71 lb in
Upper Valve Body Side Bolts | 5 N·m | 44 lb in
Valve Body Bolt | 10 N·m | 89 lb in