Crankshaft Rear Oil Seal and Housing Removal. Chevrolet Metro 1998

For 1990-2009 cars

1. Remove the five rear main seal housing bolts.
2. Remove the rear main seal housing.
3. Using a hammer and a drift, carefully remove the rear main seal from the rear main seal housing.
4. Carefully install the new rear main seal (1) into the rear main seal housing (2) with a hammer. Tap the rear main oil seal into place so that the end face is flush with the housing seal end face.