Oil Pan Cleaning and Inspection. Chevrolet Metro 1998

For 1990-2009 cars

•

- Clean the oil pan mating surface.

•

- Clean the oil pan. Remove all the sludge and the oil deposits.

•

- Inspect the threads for the engine oil drain plug.

•

- Inspect the oil pan for cracking near the pan rail and the transmission mounting points.

•

- Inspect the oil pan for cracking resulting from impact or flying road debris.

•

- Repair or replace the oil pan as necessary.