ABS Components. Chevrolet Metro 2001

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Antilock Brake System (ABS) Motor Pack Assembly (With ABS) | The left side of the rear engine compartment, attached to the brake master cylinder | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Brake Fluid Level Switch | In the brake-fluid reservoir | -- | Hydraulic Brake Connector End Views in Hydraulic Brakes
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Electronic Brake Control Module (EBCM) (With ABS) | Behind the left IP, above the junction block | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Fuse Box | The left side of the engine compartment, mounted on the left inner side of the fender, behind the relay box | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Instrument Panel Cluster Assembly | The left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Lamp Driver Relay (With ABS) | Behind the left side of the IP, to the left of the steering column, near the electronic brake control module (EBCM) | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Left Front Wheel Speed Sensor (With ABS) | Mounted in the left front side of the steering knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Left Rear Wheel Speed Sensor (With ABS) | Mounted in the left rear side of the suspension knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Left Front ABS Solenoid | The left rear of the engine compartment, attached to the ABS motor-pack assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Relay Box | The left front engine compartment, near the battery | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Right Front Wheel Speed Sensor (With ABS) | Mounted in the right front side of the steering knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Right Rear Wheel Speed Sensor (With ABS) | Mounted in the right rear side of the suspension knuckle | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Right Front ABS Solenoid | The left rear side of the engine compartment, attached to the ABS motor-pack assembly | Antilock Brake System Component Views | Antilock Brake System Connector End Views
Stoplamp Switch | The top of the brake pedal | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
C114 (2 Cavities) (With ABS) | The main harness to the jumper harness of the speed sensor for the left front wheel, in the left rear engine compartment, near the strut tower | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C115 (2 Cavities) (With ABS) | The main harness to the jumper harness of the speed sensor for the right front wheel, in the right rear side of the engine compartment near the strut tower | Harness Routing Views in Wiring Systems | --
C200 (12 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (14 Cavities) | The main harness to the floor harness, behind the left side of the IP, near the junction block | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C304 (2 Cavities) (With ABS) | The floor harness to the speed sensor jumper harness for the right rear wheel , under the right side of the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C305 (2 Cavities) (With ABS) | The floor harness to the speed sensor jumper harness for the left rear wheel, under the left side of the rear passenger seat | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G102 | The left front side of the engine compartment on the left-front inner fender near the battery | Harness Routing Views in Wiring Systems | --
G201 | Behind the left side of the kick panel | Harness Routing Views in Wiring Systems | --
P100 (With ABS) | The left rear side of the engine compartment on the strut tower | -- | --
P101 (With ABS) | The right rear side of the engine compartment on the strut tower | -- | --
P200 | The left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in Wiring Systems | --
P301 (With ABS) | Under the right side of the rear passenger seat | -- | --
P302 (With ABS) | Under the left side of the rear passenger seat | -- | --
S124 (With ABS) | The main harness, approximately 5 cm (2 in) from the front of the ABS solenoids breakout | -- | --
S206 (With ABS) | The main harness, approximately 22 cm (9 in) from the stoplamp-switch connector breakout | -- | --
S207 | The main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S208 (With ABS) | The main harness, approximately 12 (5 in) cm from the G201 breakout | -- | --
S209 | The main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S213 | The main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S215 (With ABS) | The main harness, approximately 4 cm (2 in) from the breakout of the junction-block connector C6 | -- | --
S223 | The main harness, approximately 10 cm (4 in) from P200 | -- | --
S241 | The IP harness, approximately 5 cm (2 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S242 | The IP harness, at the breakout of the IP cluster assembly connector C3 | Harness Routing Views in Wiring Systems | --
S247 | The main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S249 | The IP harness, approximately 1 cm (0.375 in) from the breakout of the IP cluster assembly connector C2 | Harness Routing Views in Wiring Systems | --
S251 (With ABS) | The main harness, approximately 5 cm (2 in) from P200 | -- | --