Synchronizers. Chevrolet Metro 1998

For 1990-2009 cars

The low speed synchronizer mounts on the countershaft. The low speed synchronizer will engage with either the countershaft 1st gear or the countershaft 2nd gear. The high speed synchronizer mounts on the input shaft. The high speed synchronizer will engage with either the input shaft 3rd gear or the input shaft 4th gear. The 5th speed synchronizer mounts on the input shaft. The 5th speed synchronizer engages with the input shaft 5th gear. The countershaft meshes with and turns the ring gear of the differential assembly that supplies power to the drive axles.