Tachometer Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument panel cluster. Refer to Instrument Cluster Replacement .
2. Push on the tabs in order to remove the cluster lens (10) and the bezel (9) from the cluster housing (6).
3. Remove the 3 screws (1) that retain the tachometer.
4. Remove the tachometer (8) from the cluster housing (6).

### Installation Procedure

1. Install the tachometer (8) to the cluster housing (6).
2. Secure the tachometer with the 3 screws (1).
3. Install the cluster lens (10) and the bezel (9) to the cluster housing (6).
4. Install the instrument panel cluster. Refer to Instrument Cluster Replacement .