Front Side Door Weatherstrip Replacement. Chevrolet Metro 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the outside rearview mirror. Refer to Manual Mirror Replacement .
2. Remove the 3 screws (2) and the front door rear molding (1) from the front door (3).
3. Partially lower the door window weather strip (2) in order to gain the necessary clearance in order to remove the door opening weather strip (1).
4. Remove the 2 plastic retainers that retain the front door opening molding (1).
5. Pull the molding (1) from the door (2).

### Installation Procedure

1. Install the door opening weather strip (1). Secure the molding with the 2 plastic retainers.
2. Install the door window weather strip (2) to the door (3).
3. Install the front door rear molding (1) to the door (3). Secure the molding with the 3 screws (2).
4. Install the outside rearview mirror. Refer to Manual Mirror Replacement .