Emission Hose Routing Diagram. Chevrolet Metro 1998

For 1990-2009 cars

#### Chevrolet Metro 1.0L (VIN 6)

(1) | EVAP Canister Vent Solenoid (Air Valve)
(2) | EVAP Canister
(3) | Fuel Tank Pressure Control Valve
(4) | EGR Valve
(5) | EGR Pressure Transducer
(6) | EGR Bypass Valve (Diagnostic Valve)
(7) | EGR Solenoid Vacuum Valve (Regulator Solenoid Valve)
(8) | EVAP Canister Surge Tank
(9) | EVAP Canister Purge Valve
(10) | EVAP Tank Pressure Control Solenoid Vacuum Valve
(11) | MAP Sensor