Electronic Brake Control Relay Replacement. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

1. Open the hood.
2. Remove the underhood Electrical Center cover.
3. Remove the Electronic Brake Control Relay (2) from the underhood electrical center (1).

### Installation Procedure

1. Install the Electronic Brake Control Relay (2) into the underhood electrical center (1).
2. Install the underhood Electrical Center cover.
3. Close the hood.
4. Perform the Diagnostic System Check - ABS .