Input Shaft Support Replacement. Chevrolet Nubira (Delta) 2010

For 1990-2009 cars

Callout | Component Name
--- | ---

1

3-5 Reverse and 4-5-6 Clutch Fluid Seals (Qty: 4)

Tip

• | Discard the fluid seals. They are not reusable.

• | Refer to 3-5-Reverse and 4-5-6 Clutch Fluid Seal Ring Replacement.

2 | Input Shaft Support Bolts M6 x 50 (Qty: 3) Caution: Refer to Fastener Caution in the Preface section. Tighten 12 N·m (106 lb in)
3 | Input Shaft Support Tip Inspect the support for wear, damage or porosity.