Automatic Transmission Components. Chevrolet PJJ 2000

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
1-2 Shift Solenoid Valve | In transmission valve body | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
2-3 Shift Solenoid Valve | In transmission valve body | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
Automatic Transmission | LH side of the engine compartment | -- | Automatic Transmission Inline Harness Connector End View
Automatic Transmission Fluid Temperature Sensor | In transmission valve body | -- | --
Brake Switch | Lower RH IP, below steering column | Cruise Control Component Views in Cruise Control | --
Fuse Block | LH end of IP tie bar | Electrical Center Identification in Wiring Systems | --
Powertrain Control Module (PCM) | RH front of car behind fascia | Engine Controls Component Views in Engine Controls | PCM Connector End Views in Engine Controls
Torque Converter Clutch Pulse Width Modulation Solenoid Valve | In the transmission valve body | Automatic Transmission Electronic Component Views | --
Torque Converter Clutch Solenoid Valve | In the transmission valve body | Automatic Transmission Electronic Component Views | Automatic Transmission Internal Connector End Views
Vehicle Speed Sensor | LH rear of the transmission | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
C100 (38 cavities) | LH rear side of engine compartment | Harness Routing Views in Wiring Systems | Inline Connector End Views in Wiring Systems
P201 | LH lower IP below steering column | Harness Routing Views in Wiring Systems | --
S107 | In the engine harness, front left side of engine, approximately 34 cm (13 in) from the engine comaprtment fuse/relay center | -- | --
S214 | In the dash harness, approximately 18 cm (7 in) from the electronic brake control module connector C2 | -- | --
S242 | In the dash harness, approximately 84 cm (33 in) from P201, toward the data link connector | -- | --