Transmission Floor Shift Control Indicator Lamp Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the console trim plate. Refer to Trim Plate Replacement - Console.
2. Disconnect electrical connectors.
3. Remove the gear shift handle.
4. Remove the console. Refer to Console Replacement.
5. Disconnect the transmission console socket (2) by twisting counter clockwise.
6. Pull the bulb (3) from the socket to remove.

### Installation Procedure

1. Install the transmission console lamp socket (3).
2. Install the console. Refer to Console Replacement.
3. Install the gear shift handle.
4. Connect electrical connectors.
5. Install the console trim plate. Refer to Trim Plate Replacement - Console.