Scan Tool Data List. Chevrolet PJJ 2000

For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition On/Engine Off
Battery Voltage | BCM Data | Volts | 12.0 Volts
Ignition 1 | BCM Data | On/Off | On
Accessory | BCM Data | On/Off | On
Key In Ignition | BCM Data | On/Off | On
Traction Switch | BCM Data | On/Off | Off
A/C Request | BCM Data | Yes/No | No
Rear Defog Switch | BCM Data | On/Off | Off
Park Brake Switch | BCM Data | On/Off | Off
Brake Fluid Level Switch | BCM Data | On/Off | Off
Low Coolant Level | BCM Data | On/Off | Off
Rear Defog Relay | BCM Data | On/Off | Off
Rear Defog Relay Feedback | BCM Data | Active/Inactive | Inactive
Park (BTSI) Relay | BCM Data | On/Off | On
Park (BTSI) Relay Feedback | BCM Data | Active/Inactive | Active
Panic Horn Relay | BCM Data | On/Off | Off
Panic Horn Relay Feedback | BCM Data | Active/Inactive | Inactive
Last 4 Dig of GM Part # | ID Information | -- | 4014
Model Year | ID Information | -- | 2000
Year Module Built | ID Information | -- | 2000
Calibration ID | ID Information | -- | 00000000