Scan Tool Data List. Chevrolet PJJ 2000

For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition On, Engine Off
DRL Relay | Lamp Status | On/Off | Off
DRL Relay Feedback | Lamp Status | Active/Inactive | Inactive
Park Lamp Input | Lamp Status | On/Off | Off
Low Beam Feedback | Lamp Status | Volts | 12.00 Volts
High Beam Feedback | Lamp Status | Volts | 12.00 Volts
Front Fog Lamp Switch | Lamp Status | On/Off | Off
Front Fog Lamp Relay | Lamp Status | On/Off | Off
Fog Lamp Relay Feedback | Lamp Status | Active/Inactive | Inactive
Interior Dim Pot | Lamp Status | Volts | 0.00 Volts
Interior Lamp Output | Lamp Status | On/Off | Off
Interior Lamp Feedback | Lamp Status | Active/Inactive | Inactive
Driver Door Ajar Switch | Lamp Status | On/Off | Off
Passenger Door Ajar Switch | Lamp Status | On/Off | Off
Inadvert. Power Output | Lamp Status | On/Off | On
Inadvert. Power Feedback | Lamp Status | Active/Inactive | Active
Cargo Lamp On | Lamp Status | On/Off | Off