Passenger Front EZ Entry Seat Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the driver or passenger front seat. Refer to Seat Replacement
2. Place the front seat on a clean, dry, non - abrasive surface.
3. Remove the front seat back from the seat cushion. Refer to Front Seat Back Replacement
4. Disconnect the seat pad and cover Jardinieres (1) from the seat cushion frame (2).
5. Remove the seat pad and cover assembly (1) from the seat frame (3).

### Installation Procedure

1. Install the seat pad and cover assembly (1) to the seat frame (3).
2. Install the seat pad and cover Jardinieres (2) to the seat frame.
3. Attach the front seat back to the seat cushion. Refer to Front Seat Back Replacement
4. Install the driver or passenger front seat into vehicle. Refer to Seat Replacement