Engine Controls Components. Chevrolet PJJ 2000

For 1990-2009 cars

Component | Location | Locator View | Connector End View
--- | --- | --- | ---
Automatic Transaxle | On the lower rear of the engine | -- | AT Inline Harness Connector End View in Transmission Transaxle
Camshaft Position (CMP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Crankshaft Position (CKP) Sensor | In the lower front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Data Link Connector (DLC) | On the left side of the IP | Engine Controls Component Views | Engine Controls Connector End Views
Engine Coolant Level Switch | In the right side of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
Engine Coolant Temperature (ECT) Sensor | On the top rear of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Engine Oil Pressure Sensor | On the top left of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission Canister Purge Valve | On the lower front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Evaporative Emission Canister Vent Solenoid | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Injectors | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Pump Relay | In the Underhood Fuse/Relay Center | -- | --
Fuel Tank Module | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Fuel Tank Pressure Sensor | Under the rear of the vehicle | Engine Controls Component Views | Engine Controls Connector End Views
Fuse Block | On the LH end of IP tie bar | Power and Grounding Component Views in Wiring Systems | --
Generator | On the lower front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Idle Air Control (IAC) Valve | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Coils | On the rear of engine | Engine Controls Component Views | Engine Controls Connector End Views
Ignition Control Module | On the top left of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Instrument Cluster | On the left side of the IP | Instrument Cluster Component Views in Instrument Panel Gauges and Console | Instrument Cluster Connector End Views in Instrument Panel Gauges and Console
Intake Air Temperature (IAT) Sensor | On the top left side of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
Knock Sensor | On the top left side of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Manifold Absolute Pressure (MAP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Powertrain Control Module | Inside of the RF fender, in front of the wheel | Engine Controls Component Views | Engine Controls Connector End Views
Pre Converter Oxygen Sensor (O2S 1) | In the exhaust manifold | Engine Controls Component Views | Engine Controls Connector End Views
RH Cooling Fan Motor | In the front of the engine compartment | Engine Controls Component Views | Engine Controls Connector End Views
Throttle Position (TP) Sensor | On the top front of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Park/Neutral Position Switch | On the left side of the engine | Engine Controls Component Views | Engine Controls Connector End Views
Underhood Fuse/Relay Center | In the left side of the engine compartment | Power and Grounding Component Views in Wiring Systems | --
Vehicle Speed Sensor (VSS) | At the rear of the engine/transaxle | Engine Controls Component Views | Engine Controls Connector End Views
C100 | On the left side of the engine compartment | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C102 (20 cavity) | On the left side of the engine | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C200 (18 cavity) | Below the left side of the IP, near the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C300 (10 cavity) | Below the left side of the IP, near the steering column | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C413 (16 cavity) | Under the rear of the vehicle | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G102 | On the front of the engine | Harness Routing Views in Wiring Systems | --
G102 | On the lower front of the engine | Harness Routing Views in Wiring Systems | --
G103 | On the lower front of the engine | Harness Routing Views in Wiring Systems | --
G201 | On the left side of the IP | Harness Routing Views in Wiring Systems | --
G301 | On the left side of the passenger compartment | Harness Routing Views in Wiring Systems | --
P100 | In the rear of the engine compartment | Harness Routing Views in Wiring Systems | --
P200 | In the rear of the engine compartment | Harness Routing Views in Wiring Systems | --
S101 | In the injector harness, approximately 16 cm (6.3 in) from C130, towards the injectors | Harness Routing Views in Wiring Systems | --
S102 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S103 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S104 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --
S105 | In the engine harness, approximately 15 cm (5.9 in) from P100, towards the PCM | -- | --