Power Steering Rack and Pinion Gear Disassembled View. Chevrolet PJJ 2000

For 1990-2009 cars

#### Power Rack and Pinion-End Take Off

(1) | Tie Rod and End Housing Seal
(2) | Hexagon Slotted Nut
(3) | Cotter Pin
(4) | Outer Tie Rod Assembly
(5) | Hex Jam Nut
(6) | Tie Rod End Clamp
(7) | Rack and Pinion Boot
(8) | Boot Retaining Clamp
(9) | Inner Tie Rod Assembly
(10) | Shock Dampener Ring
(11) | Manifold Gasket
(12) | Control Valve and Manifold Assembly
(13) | Pan HD 6-Lobed Soc (M6x1) Screws
(14) | Seal Adapter
(15) | O-ring Seals
(16) | Cylinder Line (RT)
(17) | Cylinder Line (LT)
(18) | Rack and Pinion Gear Assembly (Partial)
(19) | Shock Dampener Ring
(20) | Inner Tie Rod Assembly
(21) | Boot Retaining Clamp
(22) | Rack and Pinion Boot
(23) | Tie Rod End Clamp
(24) | Cotter Pin
(25) | Hexagon Slotted Nut
(26) | Tie Rod and End Housing Seal
(27) | Outer Tie Rod Assembly
(28) | Hex Jam Nut