Fuel Tank Filler Door Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Remove the nuts (2) from the fuel tank filler door.
2. Remove the fuel tank filler door (1).
3. Remove the filler door latch. Refer to Fuel Filler Door Release Actuator Replacement.

### Installation Procedure

1. Install the filler door latch. Refer to Fuel Filler Door Release Actuator Replacement .
2. Install the nuts (2) to the filler door (1).
3. Install the fuel tank filler door .

Tighten
Tighten the nuts to 2 N·m (24 lb in).