Power and Grounding Connector End Views. Chevrolet PJJ 2000

For 1990-2009 cars

Table 1: | Cigar Lighter
Table 2: | Ignition Switch C1
Table 3: | Ignition Switch C2

#### Cigar Lighter

Connector Part Information

• | 12047699

• | 2-Way Cigar Lighter (GRY)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | ORN | 40 | Fuse Output (Battery)
B | BLK | 150 | Ground

#### Ignition Switch C1

Connector Part Information

• | 12129842

• | 6-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | PNK | 3 | Ignition Switch Output Ignition 1
B | ORN | 300 | Ignition Switch Output Ignition 3
C | YEL | 5 | Ignition Switch Output Ignition
D | WHT | 1390 | Ignition Switch Output (OFF/RUN/CRANK)
E | BLK | 150 | Ground
F | BLK | 150 | Ground

#### Ignition Switch C2

Connector Part Information

• | 12162229

• | 6-Way F Metri-Pack Mixed Series (BLK)

Pin | Wire Color | Circuit No. | Function
--- | --- | --- | ---
A | BRN | 4 | Ignition Switch Output (Accessory)
B | RED | 242 | Fuse Output (Battery)
C | RED | 242 | Fuse Output (Battery)
D | BLK | 1350 | Ground
E | -- | -- | Not Used
F | LT GRN | 80 | Key Reminder Switch Signal