Sunroof Opening Trim Finish Lace Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

1. Pull the sunroof opening trim lace away from the headliner.
2. Beginning at the joint, pull the sunroof opening trim lace until the entire weatherstrip is removed.

### Installation Procedure

1. Start the joint on the center of the left side of the opening. Fully seat the sunroof opening trim lace into place around the sunroof opening.
2. Take care to fully seat the lace into the corners.