Scan Tool Data List. Chevrolet PJJ 2000

For 1990-2009 cars

Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
--- | --- | --- | ---
Ignition On/Engine Off
Trip Reset Switch | Inputs | Active/Inactive | Inactive
Ignition 1 | Inputs | On/Off | On
Ignition 1 | Inputs | Volts | 12.0 Volts
Oil Pressure Lamp | Lamp Status | On/Off | On
ABS Lamp | Lamp Status | On/Off | Off
Traction Off Lamp | Lamp Status | On/Off | Off
Low Fuel Lamp | Lamp Status | On/Off | Off
Volt Lamp | Lamp Status | On/Off | On
Upshift Lamp | Lamp Status | On/Off | Off
High Coolant Temp Lamp | Lamp Status | On/Off | Off
Service Vehicle Soon Lamp | Lamp Status | On/Off | Off
Low Coolant Lamp | Lamp Status | On/Off | Off
SIR Lamp | Lamp Status | On/Off | Off
Seat Belt Lamp | Lamp Status | On/Off | Off
High Beam Lamp | Lamp Status | On/Off | Off
Brake Lamp | Lamp Status | On/Off | Off
Gear Range Status | Gear Status | Varies | Park