Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Coolant Pump Cover to Engine Block Bolts 2.4L (LD9) | 26 N·m | 19 lb ft
Coolant Pump to Coolant Pump Cover Bolts 2.4L (LD9) | 14 N·m | 124 lb in
Coolant Pump to Timing Chain Housing Nuts 2.4L (LD9) | 26 N·m | 19 lb ft
Engine Cooling Fan Bolt | 6 N·m | 53 lb in
Radiator Outlet Pipe to Coolant Pump Cover Bolts 2.4L (LD9) | 14 N·m | 124 lb in
Radiator Outlet Pipe to Engine Oil Pan Bolt 2.4L (LD9) | 25 N·m | 18 lb ft
Radiator Surge Tank Cap | 4 N·m | 35 lb in
Radiator Upper Mount Bolt | 10 N·m | 89 lb in
Surge Tank Inlet Hose Clip | 10 N·m | 89 lb in
Transaxle Oil Cooler Line Fittings at Radiator | 36 N·m | 27 lb ft
Transaxle Oil Cooler Line Bracket | 10 N·m | 89 lb in