Armrest Bracket Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Trim Panel Replacement - Door.
2. Remove the rivets (3) which retain the front door armrest hanger plate (1).
3. Remove the front door armrest hanger plate (1).

### Installation Procedure

1. Install the front door armrest hanger plate (1).
2. Install the rivets (3) to the front door hanger plate.
3. Install the front door trim panel. Refer to Trim Panel Replacement - Door.