Diagnostic Trouble Code (DTC) List. Chevrolet PJJ 2000

For 1990-2009 cars

Description | Module
--- | ---
DTC C1214 System Relay Contact or Coil Circuit Open | EBCM
DTC C1217 Pump Motor Shorted to Ground | EBCM
DTC C1218 Pump Motor Circuit Shorted to Voltage or Motor Ground Open | EBCM
DTC C1221 LF Wheel Speed Sensor Input Signal is 0 | EBCM
DTC C1222 RF Wheel Speed Sensor Input Signal is 0 | EBCM
DTC C1223 LR Wheel Speed Sensor Input Signal is 0 | EBCM
DTC C1224 RR Wheel Speed Sensor Input Signal is 0 | EBCM
DTC C1225 LF Excessive Wheel Speed Variation | EBCM
DTC C1226 RF Excessive Wheel Speed Variation | EBCM
DTC C1227 LR Excessive Wheel Speed Variation | EBCM
DTC C1228 RR Excessive Wheel Speed Variation | EBCM
DTC C1232 LF Wheel Speed Circuit Open or Shorted | EBCM
DTC C1233 RF Wheel Speed Circuit Open or Shorted | EBCM
DTC C1234 LR Wheel Speed Circuit Open or Shorted | EBCM
DTC C1235 RR Wheel Speed Circuit Open or Shorted | EBCM
DTC C1236 Low System Supply Voltage | EBCM
DTC C1237 High System Supply Voltage | EBCM
DTC C1242 Pump Motor Circuit Open | EBCM
DTC C1243 BPMV Pump Motor Stalled | EBCM
DTC C1254 Abnormal Shutdown Detected | EBCM
DTC C1255 EBCM Internal Malfunction | EBCM
DTC C1256 EBCM Internal Malfunction | EBCM
DTC C1261 LF Inlet Valve Solenoid Malfunction | EBCM
DTC C1262 LF Outlet Valve Solenoid Malfunction | EBCM
DTC C1263 RF Inlet Valve Solenoid Malfunction | EBCM
DTC C1264 RF Outlet Valve Solenoid Malfunction | EBCM
DTC C1265 LR Inlet Valve Solenoid Malfunction | EBCM
DTC C1266 LR Outlet Valve Solenoid Malfunction | EBCM
DTC C1267 RR Inlet Valve Solenoid Malfunction | EBCM
DTC C1268 RR Outlet Valve Solenoid Malfunction | EBCM
DTC C1275 PCM Requested ETS to Be Disabled | EBCM
DTC C1278 ETS Temporarily Inhibited By PCM | EBCM
DTC C1295 Brake Lamp Switch Circuit Open | EBCM
DTC C1298 PCM Class 2 Serial Data Link Malfunction | EBCM
DTC U1000 Class 2 Communication Malfunction in Data Link Communications | EBCM
DTC U1016 Loss of Communications with PCM in Data Link Communications | EBCM
DTC U1300 Class 2 Data Link Low in Data Link Communications | EBCM
DTC U1301 Class 2 Data Link High in Data Link Communications | EBCM