Instrument Cluster Indicator Lamp Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

### Removal Procedure

Use the following procedure in order to change any instrument panel bulb, instrument warning bulb, or cluster illumination bulb.

1. Remove the instrument panel cluster. Refer to IP Cluster Replacement.
2. Twist the bulb/socket assembly counterclockwise in order to remove the bulb/socket assembly.

### Installation Procedure

1. Install the bulb into the socket.
2. Install the socket into the cluster.

Turn the socket clockwise in order to tighten the socket.

3. Install the cluster into the instrument panel. Refer to IP Cluster Replacement.