Scan Tool Output Controls. Chevrolet PJJ 2001

For 1990-2009 cars

#### Body Control Module (BCM)

Scan Tool Output Control | Additional Menu Selection(s) | Description
--- | --- | ---
Cluster Dimming | Light Test | The BCM actuates the instrument panel lamp output when you select ON. The instrument panel lamps should illuminate for 5 seconds.
Inadvertent Power | Inadvertent Power | The BCM deactivates the INADVERTENT POWER output when you select OFF. The foot well, IP compartment, rear compartment, vanity mirror, and courtesy lamps should be inoperative.
Interior Lamps | Light Test | The BCM actuates the interior lamp control for 5 seconds when you select ON. The foot well, and courtesy lamps should illuminate for 5 seconds.