Fastener Tightening Specifications. Chevrolet PJJ 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Hose to Caliper Bolt | 44 N·m | 32 lb ft
Brake Pedal Bracket to Support Brace Nuts | 10 N·m | 89 lb in
Brake Pipes at Master Cylinder | 23 N·m | 17 lb ft
Brake Pipes at Proportioning Valve | 27 N·m | 20 lb ft
Brake Pipe Tube Nuts | 23 N·m | 17 lb ft
Caliper Bleeder Screw | 13 N·m | 115 lb in
Caliper Mounting Bolts | 51 N·m | 38 lb ft
Master Cylinder Mounting Nuts | 27 N·m | 20 lb ft
Master Cylinder Reservoir Screws | 2 N·m | 18 lb in
Vacuum Brake Booster to Pedal Bracket Nuts | 2 N·m | 18 lb in
Wheel Cylinder Bleeder Screw | 7 N·m | 62 lb in