Rear Compartment Lid Latch Release Cable Replacement. Chevrolet PJJ 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the handle cover from the compartment lid release.
2. Remove the remote release cable (2) from the remote release handle (1).
3. Unclip the cable door at the top of the lock release box (2).
4. Remove the remote release cable (1) from the lock release box (2).

### Installation Procedure

1. Route the remote release cable (2).
2. Install the remote release cable (2) to the remote release handle (1).
3. Install the release handle cover.
4. Install the remote release cable (1) to the lock release box (2).
5. Press and secure the cable door at the top of the lock release box.