Rear Quarter Trim Panel Replacement. Chevrolet PJJ 2001

For 1990-2009 cars

## Rear Quarter Trim Panel Replacement 2 Door

### Removal Procedure

1. Remove the rear seatback assembly. Refer to Seat Back Replacement - Rear.
2. Remove the coat hook. Refer to Coat Hook Replacement.
3. Remove the quarter panel extension retainer (1).
4. Remove the quarter trim panel extension (2).
5. Remove the seat belt opening escutcheon (1).
6. Remove side belt anchor bolt from the front seat retractor. Refer to the following procedures:

• | Seat Belt Retractor Replacement - Left Front (Sedan) in Seat Belts.

• | Seat Belt Retractor Replacement - Left Front (Coupe) in Seat Belts.

• | Seat Belt Retractor Replacement - Right Front (Sedan) in Seat Belts.

• | Seat Belt Retractor Replacement - Right Front (Coupe) in Seat Belts.

7. Disengage the fasteners.
8. Remove the quarter trim panel (1).
9. Remove the front seat retractor side belt (2) through the opening in the quarter trim panel (1).
10. Remove the rear seat outer retractor side belt (3) through the slot in the quarter trim panel (1).

### Installation Procedure

1. Install the rear seat outer retractor side belt (3) through the slot in the quarter trim panel (1).
2. Install the front seat retractor side belt (2) through the opening in the quarter trim panel.
3. Install the quarter trim panel (1).
4. Install the side belt anchor bolt to the front seat retractor. Refer to the following procedures:

• | Seat Belt Retractor Replacement - Left Front (Sedan) in Seat Belts.

• | Seat Belt Retractor Replacement - Left Front (Coupe) in Seat Belts.

• | Seat Belt Retractor Replacement - Right Front (Sedan) in Seat Belts.

• | Seat Belt Retractor Replacement - Right Front (Coupe) in Seat Belts.

5. Install the seat belt opening escutcheon (1).
6. Install the quarter trim panel extension (2).
7. Install the quarter trim panel extension retainer (1).
8. Install the coat hook (2). Refer to Coat Hook Replacement.
9. Install the rear seatback assembly. Refer to Seat Back Replacement - Rear.

## Rear Quarter Trim Panel Replacement 4 Door

### Removal Procedure

1. Remove the rear seatback assembly. Refer to Seat Back Replacement - Rear in Seats.
2. Disengage the upper quarter trim panel fasteners.
3. Remove the upper quarter trim panel (1).
4. Remove the lower quarter trim panel retainer (1).
5. Disengage the lower quarter trim panel fasteners.
6. Remove the lower quarter trim panel (2).

### Installation Procedure

1. Install the lower quarter trim panel (2).
2. Install the lower quarter trim panel retainer (1).
3. Install the upper quarter trim panel (1).
4. Install the rear seatback assembly. Refer to Seat Back Replacement - Rear in Seats.