Symptoms. Chevrolet PJJ 2000

For 1990-2009 cars

Important: The following steps must be completed before using the symptom tables.

1. Perform the Diagnostic System Check - Charging System before using the Symptom Tables in order to verify that all of the following are true:

• | There are no DTCs set.

• | The control module(s) can communicate via the serial data link.

2. Review the system operation in order to familiarize yourself with the system functions. Refer to the Starting System Description, the Starting System Circuit Description, the Charging System Description and the Charging System Circuit Description.

### Visual/Physical Inspection

• | Inspect for aftermarket devices which could affect the operation of the Starting and Charging System. Refer to Checking Aftermarket Accessories in Wiring Systems.

• | Inspect the easily accessible or visible system components for obvious damage or conditions which could cause the symptom.

### Intermittent

Faulty electrical connections or wiring may be the cause of intermittent conditions. Refer to Testing For Poor Connections in Wiring Systems.

### Symptom List

Refer to a symptom diagnostic procedure from the following list in order to diagnose the symptom:

• | Starter Solenoid Does Not Click

• | Starter Solenoid Clicks/Engine Does Not Crank

• | Engine Cranks Slowly

• | Battery Inspection/Test

• | Charge Indicator Always On

• | Charge Indicator Inoperative