For 1990-2009 cars

## Front Side Door Window Switch Replacement Right Front Door

### Removal Procedure

1. Using a taped flat bladed tool, gently pry the front side door accessory switch mounting plate (2) from the front side door trim (1).
2. Disconnect the front side door power window switch electrical connector (2).
3. Remove the front side door power window switch (2) from the mounting plate (3) by releasing the tabs (4).

### Installation Procedure

1. Install the front side door power window switch (2) to the front side door accessory switch mounting plate (3). Ensure that the retaining tabs (4) are completely engaged.
2. Connect the front side door power window switch electrical connector (2).
3. Install the front side door accessory switch mounting plate (1) to the front side door trim (2).