For 1990-2009 cars

#### ABS Data

Ignition ON, Engine OFF, Transmission in Neutral or Park, and Brake Unapplied
Scan Tool Parameter | Data List | Units Displayed | Typical Data Value
ABS Active | ABS | No/Yes | No
ABS Warning Lamp | ABS | On/Off | Off
Brake Switch | ABS | Applied/Released | Released
Ignition Voltage | ABS | Volts | Varies
Left Front Wheel Speed | ABS | mph/km/h | 0
Left Rear Wheel Speed | ABS | mph/km/h | 0
LF Solenoid Commanded | ABS | Active/Inactive | Inactive
LF Solenoid Monitor | ABS | Active/Inactive | Inactive
LR Solenoid Commanded | ABS | Active/Inactive | Inactive
LR Solenoid Monitor | ABS | Active/Inactive | Inactive
Pump Motor Commanded | ABS | On/Off | Off
Pump Motor Monitor | ABS | On/Off | Off
RF Solenoid Commanded | ABS | Active/Inactive | Inactive
RF Solenoid Monitor | ABS | Active/Inactive | Inactive
Right Front Wheel Speed | ABS | mph/km/h | 0
Right Rear Wheel Speed | ABS | mph/km/h | 0
RR Solenoid Commanded | ABS | Active/Inactive | Inactive
RR Solenoid Monitor | ABS | Active/Inactive | Inactive
Valve Relay State | ABS | On/Off | On