For 1990-2009 cars

# Info - Current Model Year Goodwrench Transmission Replacement Assembly Program

Subject: | Current Model Year Goodwrench Transmission Replacement Assembly Program

Models: | 1998-2007 GM Passenger Cars and Light Duty Trucks

| 2003-2007 HUMMER H2

| 2006-2007 HUMMER H3

| with 4L30-E, 4L60-E, 4L65-E, 4L70-E, 4L80-E, 4L85-E, 6L50, 6L80, 3T40, 4T40-E, 4T45-E, 4T60-E, 4T65-E, 4T80-E or 6T70 Automatic Transmission

This bulletin is being revised to add additional model years. Also, the identification tag color for remanufactured transmissions has changed. Please discard Corporate Bulletin Number 00-07-30-009A (Section 07 -- Transmission/Transaxle).

There may be some confusion about the Goodwrench® transmission assembly program and whether a Goodwrench transmission is new or remanufactured.

It should not be assumed that a Goodwrench transmission is a remanufactured unit.

Goodwrench transmissions for the current model year are new transmission assemblies. A new Goodwrench transmission may be identified by inspecting the transmission stick-on label. The stick-on label will indicate "Manufactured by General Motors" and the identification tag is blue. A remanufactured Goodwrench transmission may be identified by inspecting the transmission stick-on label. The stick-on label will indicate "Remanufactured for General Motors" and the identification tag is black.