For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Brake Pressure Modulator Valve (BPMV) | LH rear of engine compartment, below master cylinder | Antilock Brake System Component Views in Antilock Brakes | Antilock Brake System Connector End Views in Antilock Brakes
Data Link Connector (DLC)- OBD 2 | Under LH instrument panel, attached to knee bolster | Data Link Communications Component Views | Data Link Communications Connector End Views
Data Link Connector (Underhood) | LH rear of engine compartment attached to strut tower | Data Link Communications Component Views | Data Link Communications Connector End Views
Fuse And Relay Block 1 | LH front engine compartment, left of air cleaner (ACL) | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Inflatable Restraint Sensing and Diagnostic Module (SDM) | Front center of console, below heater case | SIR Component Views in SIR | SIR Connector End Views in SIR
Instrument Cluster Assembly | LH instrument panel | Instrument Panel, Gages, and Console Component Views in Instrument Panel, Gauges and Console | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block 1 | Behind LH body hinge pillar trim panel | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Junction Block 2 | LH instrument panel, behind storage box access cover | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Junction Block 3 | Behind center instrument panel | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
Powertrain Control Module (PCM) | Front of center console, below radio | Engine Controls Component Views in Engine Controls - 1.8L | Powertrain Control Module Connector End Views in Engine Controls - 1.8L
C200 (14 cavities) | Engine main to cowl harness; behind LH body hinge pillar trim panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C201 (14 cavities) | Engine main to cowl harness; behind LH body hinge pillar trim panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C210 (16 cavities) | Instrument panel harness to cowl harness; attached to RH center instrument panel support bracket | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C211 (14 cavities) | Instrument panel harness to cowl harness; attached to RH center instrument panel support bracket | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C212 (19 cavities) | Cowl harness to engine accessory harness; attached to RH center instrument panel support bracket | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C222 (12 cavities) | Engine accessory harness to instrument panel harness; attached to LH center instrument panel support bracket | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C223 (22 cavities) | Engine accessory harness to instrument panel harness; attached to LH center instrument panel support bracket | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G103 | LH front of engine compartment, behind battery | Power and Grounding Component Views in Wiring Systems | --
G106 | Rear of engine compartment, on cylinder head | Power and Grounding Component Views in Wiring Systems | --
G200 | Behind LH body hinge pillar trim panel | Power and Grounding Component Views in Wiring Systems | --
G204 | Behind center instrument panel, on LH instrument panel support bracket | Power and Grounding Component Views in Wiring Systems | --
P100 | Rear of engine compartment, in LH inner fender | Harness Routing Views in Wiring Systems | --
P102 | Center of rear engine compartment | Harness Routing Views in Wiring Systems | --
S205 | Engine accessory harness; approximately 5 cm (1 15/16 in) from P102 | Harness Routing Views in Wiring Systems | --
S207 | Engine accessory harness; approximately 5 cm (1 15/16 in) from P102 | Harness Routing Views in Wiring Systems | --
SP251 | Cowl harness; taped to harness between C213 and blower motor resistor branches | Harness Routing Views in Wiring Systems | --
SP254 | Engine main harness; taped to harness between C200 and C203 breakouts | Harness Routing Views in Wiring Systems | --
SP255 | Instrument panel harness; top of LH instrument panel, behind instrument cluster assembly | Harness Routing Views in Wiring Systems | --
SP256 | Instrument panel harness; center of instrument panel, attached to G204 at LH center support bracket | Harness Routing Views in Wiring Systems | --
SP260 | Engine accessory harness; behind center instrument panel | Harness Routing Views in Wiring Systems | --