For 1990-2009 cars

#### Vibration or Rattling

Problem | Action
--- | ---
The system components are loose. | Tighten the loose components.
The system components are misaligned. | Align system components.
The support brackets are bent or damaged | Repair the support brackets as necessary.
The mounts are bent or damaged. | Repair the mounts as necessary
The heat shields are loose. | Tighten the heat shields.