For 1990-2009 cars

Table 1: | Inflatable Restraint (IR) Driver's Seat Module
Table 2: | Inflatable Restraint (IR) Left Front Discriminating Sensor
Table 3: | Inflatable Restraint (IR) LH Side Impact Sensor
Table 4: | Inflatable Restraint Passenger Seat Module
Table 5: | Inflatable Restraint Right Front Discriminating Sensor
Table 6: | Inflatable Restraint (IR) RH Side Impact Sensor
Table 7: | Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C1
Table 8: | Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C2
Table 9: | Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C3
Table 10: | Supplemental Restraint System (SRS) Coil C1
Table 11: | Supplemental Restraint System (SRS) Coil C3

#### Inflatable Restraint (IR) Driver's Seat Module

Connector Part Information |

• | 90980-11864

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/RED | Driver Seat High
2 | YEL/GRN | Driver Seat Low

#### Inflatable Restraint (IR) Left Front Discriminating Sensor

Connector Part Information |

• | 90980-11856

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | BRN | Left Sensor Return
2 | WHT/RED | Left Sensor Feed

#### Inflatable Restraint (IR) LH Side Impact Sensor

Connector Part Information |

• | 90980-11857

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | PNK/BLU | VUPL
2 | BLU/WHT | SSL
3 | LT GRN/BLK | FSL
4 | GRY/BLU | ESL

#### Inflatable Restraint Passenger Seat Module

Connector Part Information |

• | 90980-11864

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/RED | Passenger Seat Low
2 | YEL/GRN | Passenger Seat High

#### Inflatable Restraint Right Front Discriminating Sensor

Connector Part Information |

• | 90980-11869

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | BRN/WHT | RH Sensor Return
2 | BLK/WHT | RH Sensor Feed

#### Inflatable Restraint (IR) RH Side Impact Sensor

Connector Part Information |

• | 90980-11857

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | PNK | VUPR
2 | BLU/YEL | SSR
3 | LT GRN | FSR
4 | GRY | ESR

#### Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C1

Connector Part Information |

• | 90980-11869

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | YEL | LH Pretensioner Low
2 | YEL/BLK | LH Pretensioner High
3 - 4 | -- | Not Used
5 | YEL/RED | Driver Seat High
6 | YEL/GRN | Driver Seat Low
7 | PNK/BLU | VUPL
8 | -- | Not Used
9 | BLU/WHT | SSL
10 | LT GRN/BLK | FSL
11 | -- | Not Used
12 | GRY/BLU | ESL

#### Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C2

Connector Part Information |

• | 90980-11868

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | -- | Not Used
2 | BLK/YEL | AIR BAG Indicator Control
3 | BLK/ORN | Ignition Positive Voltage
4 | GRY | Ignition Positive Voltage
5 | BRN/WHT | RH Sensor Return
6 | BLK/WHT | RH Sensor Feed
7 | YEL/RED | Passenger Side High
8 | YEL/GRN | Passenger Side Low
9 | YEL | Driver Side Low
10 | YEL/BLK | Driver Side High
11 | WHT/RED | Left Sensor Feed
12 | BRN | Left Sensor Return
13-14 | -- | Not Used
15 | PNK/BLK | Diagnostic Request
16 | WHT/BLK | Ground
17 | WHT/BLK | Ground
18 | WHT | Serial Data Line
19-20 | -- | Not Used

#### Inflatable Restraint (IR) Sensing and Diagnostic Module (SDM) C3

Connector Part Information |

• | 90980-11867

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/GRN | Passenger Seat Low
2 | YEL/RED | Passenger Seat High
3-4 | -- | Not Used
5 | YEL/BLK | RH Pretensioner High
6 | YEL | RH Pretensioner Low
7 | GRY | ESR
8 | -- | Not Used
9 | LT GRN | FSR
10 | BLU/YEL | SSR
11 | -- | Not Used
12 | PNK | VUPR

#### Supplemental Restraint System (SRS) Coil C1

Connector Part Information |

• | 90980-11616

• | BLK

Pin | Wire Color | Function
--- | --- | ---
1-2 | -- | Not Used
3 | WHT/BLK | Ground
4 | GRN/BLK | Cruise Mode Signal
5 | WHT/BLU | Cruise On-Off Signal
6 | GRN/RED | Horn Relay Control

#### Supplemental Restraint System (SRS) Coil C3

Connector Part Information |

• | 90980-10850

• | YEL

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/BLK | Driver Side High
2 | YEL | Driver Side Low