For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Did you review the Radio/Audio System Description and Operation and perform the necessary inspections? | Go to Step 2 | Go to Symptoms - Entertainment
2 | Verify that the radio displays LOC. Does the radio display LOC? | Go to Step 3 | Go to Testing for Intermittent Conditions and Poor Connections in Wiring Systems
3 |

1. Remove the DOME and CIG fuses for one minute.
2. Reinstall the fuses.

Does the radio continue to display LOC?

Go to Step 4

Go to Step 5

4 | Replace the radio. Refer to Radio Replacement . Did you replace the radio? | Go to Step 5 | --
5 | Operate the system in order to verify the repair. Did you correct the condition? | System OK | Go to Step 3