For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Front or Rear Side Door Check Bolts | 5.5 N·m | 49 lb in
Front or Rear Side Door Hinge to Door Jamb Bolts | 25 N·m | 19 lb ft
Front or Rear Side Door Lock Bolt | 5 N·m | 43 lb in
Front or Rear Side Door Outside Handle Bolts | 5.5 N·m | 49 lb in
Front or Rear Side Door to Hinge Bolts | 25 N·m | 19 lb ft
Front or Rear Side Door Window to Regulator Bolts | 7 N·m | 62 lb in
Front Side Door Lock Cylinder Bolt | 5.5 N·m | 49 lb in
Front Side Door Window Rear Guide Channel Bolt | 8 N·m | 71 lb in
Front Side Door Window Regulator Bolts and Nut | 8 N·m | 71 lb in
Outside Rearview Mirror Nuts | 15 N·m | 11 lb ft
Rear Side Door Window Rear Channel Bolts | 8 N·m | 71 lb in
Rear Side Door Window Regulator Bolts | 5.5 N·m | 49 lb in