For 1990-2009 cars

### Removal Procedure

1. Remove the rear window panel diagonal brace. Refer to Support Brace Replacement - Rear Compartment in Body Rear End.
2. Remove the body rear seat back trim panel (1) from the vehicle.

### Installation Procedure

1. Install the body rear seat back trim panel (1) to the vehicle.
2. Install the rear window panel diagonal brace. Refer to Support Brace Replacement - Rear Compartment in Body Rear End.