For 1990-2009 cars

Table 1: | Instrument Cluster Assembly C1
Table 2: | Instrument Cluster Assembly C2
Table 3: | Instrument Cluster Assembly C3
Table 4: | Instrument Cluster Assembly C4

#### Instrument Cluster Assembly C1

Connector Part Information |

• | 90980-11116

• | LT GRY

Pin | Wire Color | Function
--- | --- | ---
1 | -- | Not Used
2 | RED/BLU | Ignition Positive Voltage
3 | RED/YEL | MIL Lamp Control
4 - 5 | -- | Not Used
6 | LT GRN | O/D OFF Indicator Control
7 | -- | Not Used
8 | YEL | Low Fuel Indicator Control
9 | YEL/RED | Fuel Level Signal
10 | BLK/YEL | Air Bag Indicator Control

#### Instrument Cluster Assembly C2

Connector Part Information |

• | 90980-11114

• | BLU

Pin | Wire Color | Function
--- | --- | ---
1 | RED/GRN | High Beam Indicator Control
2 | GRN/BLK | Left Turn Signal
3 | BLK | Defogger Indicator Control
4 | RED/WHT | VSS Ground
5 | -- | Not Used
6 | RED/YEL | Brake Indicator Control
7 | RED/YEL | Seat Belt Indicator Control
8 | -- | Not Used
9 | PPL/WHT | Vehicle Speed Output
10 | WHT/BLU | Vehicle Speed Input
11 | WHT/RED | ABS Lamp Driver Relay Control
12 | WHT/BLK | Ground
13 | GRN/YEL | Right Turn Signal

#### Instrument Cluster Assembly C3

Connector Part Information |

• | 90980-11113

• | WHT

Pin | Wire Color | Function
--- | --- | ---
1 | WHT/GRN | Illumination Lamps Control
2 | GRN | Lights On Signal
3 | BLK | Engine Speed Output
4 - 7 | -- | Not Used
8 | RED/BLK | Ambient Air Temperature Sensor Input
9 - 11 | -- | Not Used
12 | BLK/WHT | Start Signal
13 | RED/GRN | Battery Positive Voltage
14 | -- | Not Used
15 | BRN | Ground
16 | BRN/WHT | Sensor Ground

#### Instrument Cluster Assembly C4

Connector Part Information |

• | 90980-11115

• | BRN

Pin | Wire Color | Function
--- | --- | ---
1 | YEL/GRN | Engine Coolant Temperature Signal
2 | BRN | Ground
3 | RED/WHT | Door Open Indicator Control
4 | -- | Not Used
5 | BLU/YEL | Battery Positive Voltage
6 | -- | Not Used
7 | GRN/RED | Cruise Indicator Control
8 - 9 | -- | Not Used
10 | BLK/ORN | Ignition Positive Voltage
11 | WHT | Oil Pressure Indicator Control
12 | -- | Not Used
13 | YEL | Charge Indicator Control