For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Brake Pedal Free Play | 1-6 mm | 0.04-0.24 in
Brake Pedal Height | 148.6-158.6 mm | 5.65-6.05 in
Brake Pedal Reserve Distance (Minimum) | 85 mm | 3.35 in
Brake Pipe Clearance (Minimum)

- Moving Components

19 mm

0.75 in

- Vibrating Components

13 mm

0.50 in

Hydraulic Brake Fluid | GM P/N 12377967 or equivalent DOT 3 fluid
Stoplamp Switch Clearance | 0.5-2.4 mm | 0.02-0.09 in