For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Refrigerant-134a System Capacity | 750 g | 1.65 lbs
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) | 240 ml | 8.0 fl oz
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) - Add When Replacing Compressor Plus Amount Drained From Old Compressor | 60 ml | 2.0 fl oz
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) - Add When Replacing Condenser | 60 ml | 2.0 fl oz
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) - Add When Replacing Accumulator | 60 ml | 2.0 fl oz
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) - Add When Replacing Evaporator | 60 ml | 2.0 fl oz
Refrigerant Oil Capacity - Polyalkaline Glycol (PAG) - Add When Replacing A Hose | 30 ml | 1.0 fl oz