For 1990-2009 cars

Step | Action | Value(s) | Yes | No
1 | Were you sent here from the Wiper/Washer System Check? | -- | Go to Step 2 | Go to Wiper/Washer System Check
2 |

1. Disconnect the windshield wiper/washer switch connector.
2. Turn the ignition switch to the on position.

Do the wipers continue to operate?

--

Go to Step 4

Go to Step 3

3 | Replace the windshield wiper/washer switch. Refer to Windshield Wiper and Washer Switch Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
4 | Replace the windshield wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --