For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Case-Left Drain Plug | 32 N·m | 24 lb ft
Case M10 Bolts | 60 N·m | 44 lb ft
Case M8 Bolts | 32 N·m | 23 lb ft
Differential Carrier Nut | 500 N·m | 369 lb ft
Extension Housing Bolts | 32 N·m | 23 lb ft
Extension Housing Drain Plug | 32 N·m | 23 lb ft
Extension Housing Fill Plug | 28 N·m | 21 lb ft
Flange Nut | 250 N·m | 185 lb ft
Holding Fixture J 44755 M10 Bolts | 50 N·m | 37 lb ft
Holding Fixture J 44755 M8 Bolts | 25 N·m | 18 lb ft
Output Driveshaft Housing M10 Bolts | 60 N·m | 44 lb ft
Output Driveshaft Housing M8 Bolts | 32 N·m | 23 lb ft
Output Driveshaft Nut | 505 N·m | 372 lb ft
Speed Sensor Bolt | 30 N·m | 22 lb ft
Transfer Case-to-Transaxle Bolts - in sequence | 50 N·m | 37 lb ft
Transfer Case-to-Transaxle M10 Brace Bolts | 56 N·m | 41 lb ft
Transfer Case-to-Transaxle M8 Brace Bolts | 32 N·m | 23 lb ft