For 1990-2009 cars

1. Open the sunroof sunshade by sliding rearward.
2. Loosen the 2 screws (2) which secure each side of the sunroof window (1).
3. Adjust the sunroof window laterally by moving the window to the left or the right. The distance on either side of the sunroof window and the roof should be equal.
4. Adjust the sunroof window fore/aft position by moving the window either forward or rearward.

• | The distance between the front edge of the sunroof opening and the sunroof window (2) should be between 0.0-1.5 mm (0.0-0.059 in).

• | The distance between the rear edge of the sunroof opening and the sunroof window (2) should be between 0.0-1.5 mm (0.0-0.059 in).

5. Tighten the 2 screws (2) which secure each side of the sunroof window (1).
6. Close the sunroof sunshade by sliding forward.