For 1990-2009 cars

Figure 1: |

#### I/P Assembly Components

(1) | Hazard Switch
(2) | Rear Defogger Switch
(3) | Radio
(4) | Overdrive Switch
(5) | Noise Filter
(6) | Powertrain Control Module (PCM)
(7) | Junction Block 2
(8) | Data Link Connector (DLC) OBD 2
(9) | Junction Block 1
(10) | Malfunction Indicator Lamp (MIL)

Figure 2: |

#### LH Front Door View

(1) | LH Front Window Motor
(2) | LH Outside Rear View Mirror Connector
(3) | LH Front Speaker Connector
(4) | SP550
(5) | P500
(6) | C206
(7) | C207
(8) | C219
(9) | LH Front Speaker
(10) | SP551
(11) | LH Window/Door Lock Switch Connector (w/ Power Windows)
(12) | LH Front Door Lock Actuator (w/ Power Door Locks)

Figure 3: |

#### RH Front Door View

(1) | RH Front Window Motor
(2) | RH Front Door Lock Actuator
(3) | RH Door Lock Switch (w/ Power Locks)
(4) | RH Front Window Switch (w/ Power Windows)
(5) | SP650
(6) | RH Front Speaker
(7) | C216
(8) | C215
(9) | P600
(10) | RH Front Speaker Connector
(11) | RH Outside Rear View Mirror Connector

Figure 4: |

#### Noise Filter

(1) | EVAP Canister
(2) | EVAP Pressure Switching Solenoid
(3) | Data Link Connector (DLC) OBD 2
(4) | Data Link Connector (under hood)
(5) | EFI Relay
(6) | Noise Filter (ignition)
(7) | Powertrain Control Module (PCM)