For 1990-2009 cars

#### Tilt Steering Wheel and Column Disassembled View

(1) | Steering Wheel Inflatable Restraint Module
(2) | Steering Wheel Nut
(3) | Steering Wheel
(4) | Steering Wheel Opening Cover
(5) | Steering Wheel Opening
(6) | Turn signal and Headlamp and Windshield Washer Switch with Levers and Inflatable Restraint Coil Assembly
(7) | Steering Column Lower Support Bolt
(8) | Steering Column Lower Support Nut
(9) | Steering Shaft Coupling
(10) | Steering Shaft Coupling Bolt
(11) | Steering Column Jacket with Shaft
(12) | Steering Column Lower Trim Cover
(13) | Steering Column Upper Trim Cover
(14) | Steering Wheel Opening Cover
(15) | Steering Wheel Opening

The locking energy-absorbing tilt steering column includes the following three functions in addition to the steering function:

1. In a front-end collision, the column is designed to collapse in order to minimize driver injury.
2. The ignition switch, the steering column lock, and the ignition cylinder are column mounted, allowing the steering wheel and the ignition to be locked, minimizing the chance of vehicle theft.
3. The steering column levers control the turn signal, the headlamp switch, the headlamp dimmer switch, and the windshield wiper washer switch.

In order to ensure the energy-absorbing action, use only the specified bolts and nuts and tighten to the specified torque. Apply a thin layer of grease to all friction points during assembly. Carefully handle the column during removal. Using a steering wheel puller other than the recommended, or dropping/striking/leaning on the column, can shear or loosen the plastic fasteners that keep the column rigid.

The steering column mounted turn signal and headlamp and windshield washer switch with levers and inflatable restraint coil assembly can be serviced as a complete unit. The assembly consists of the following components:

• | The turn signal and headlamp and headlamp dimmer switch (5)

• | The windshield wiper switch and the windshield washer switch (1)

• | The steering wheel inflatable restraint module coil (2)

• | The turn signal switch base (4)