For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Back-Up Lamp Switch | 20 N·m | 15 lb ft
Drain Plug | 35 N·m | 26 lb ft
Fill Plug | 35 N·m | 26 lb ft
Front Bearing Cover Bolts | 23 N·m | 17 lb ft
Intermediate Case to Front Case Bolts | 23 N·m | 17 lb ft
Main Shift Rail Detent | 65 N·m | 48 lb ft
Power Take-Off (PTO) Cover Bolts | 38 N·m | 28 lb ft
Rear Case to Front Case Bolts | 23 N·m | 17 lb ft
Reverse Idler Shaft Bolt | 23 N·m | 17 lb ft
Shift Control Housing to Front Case Bolts | 23 N·m | 17 lb ft
Shift Interlock Plate Bolts | 10 N·m | 88 lb in
Vehicle Speed Sensor Bolt | 10 N·m | 88 lb in
Vent | 10 N·m | 88 lb in
Yoke Flange Nut | 330 N·m | 244 lb ft