For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Drum Inner Diameter (Maximum) | 201 mm | 7.913 in
Drum Out-of-Round (Maximum) | 0.01 mm | 0.0004 in
Drum Roundness (Maximum) | 0.04 mm | 0.0016 in
Drum Runout (Maximum) | 0.04 mm | 0.00016 in
Drum Taper (Maximum) | 0.1 mm | 0.004 in
Lining Material Thickness (Minimum) | 1 mm | 0.039 in
Shoe and Lining Thickness (Minimum) | 3 mm | 0.12 in
Shoe to Parking Brake Lever Clearance | 0.35 mm | 0.0138 in