For 1990-2009 cars

### Tires

Tires that do not contact and grip the road equally will cause unequal braking. Ensure that all of the tires meet the following requirements:

• | Equally inflated

• | Identical in size

• | Approximately equal tread pattern for both the right side and the left side

### Vehicle Loading

A heavily loaded vehicle requires more braking effort. When a vehicle is loaded unequally, the most heavily loaded wheels require more braking power than the other wheels.

### Wheel Alignment

Misaligned wheels will cause the brakes to pull to one side. Refer to Wheel Alignment Measurement in Wheel Alignment.